##############################################################

Separate betas is things done after R10 was released,
they have versions like 1.11RC...

The Updates for R10 are accumulative so only the latest is needed.

OBSERVE !  Only works with a final R10 installation, without
other modifications

##############################################################

Engine.exe version 1.11RC3-Y3
	Support for TLED100 module (Tank LED)
	Improved timing and memory handling.


WinDb.dll/WinDb.ini version 1.11RC10X5
	ValidationType 2 with splitchar and splitchar enforced/not enforced issues fixed

	Changes to the ValidationType 2 and workorder table use

	TLED100 dispense point TCM control now works

	Improved not enforced splitchar

	Database connect/memory leaks issues combined with many TCM tanks on PC's with "real-time" performance issues fixed

	Improved Printing and Printing logging

	Improved and adjustable Reel-Pump control timing

	Supports
	  Multiples lines with the same LineNo as long as each line has unique part numbers.

	  Without line numbers as long as each record has a unique part number

          Transaction verification ON/OFF in ini file

	  Transaction verification set to 0 now shows NOT_ACTIVE  in the start up section of WinDb.log

	  Use of start print control sequence and cancel print control sequence if the dispense stop
	  code is not 0. The two parameters PrintCsScNotZero= and PrintCsCancel= specifies it and are given
	  in ascci hex code like 1B34  ( hex 1B and 34). If PrintCsScNotZero=0 this feature is disabled

	  Try-Catch-Wait-Retry sending a print to a printer controlled by the parameters
	    PmPrintRetries=
	    PmPrintRetryDelay=

	  Workorder.line where a set splitchar is missing.
	   If WinDb service is set to use a splitcharacter but that splitcharacter is missing in a
	   transaction the used work order is stored as Work order instead of as Line number and
	   the Line number is set to "Splitchar missing"

           If parameter EnforceSplitChar= is set to 0 the whole input is validated against the workorder database
	   as if WinDb service was set to not use splitchar. If EnforceSplitChar=  is set to 1 and the splitchar
	   is missing in the input the result is NOT_VALID.

	  Disable printing when stop code is not 0

	Reel array update time now in minutes ( min 1 minute, default 2 minutes) to reduce network load.

	WinDb service tank control with only discrete sensor fixed.


Lang.lan version R11RC1 190927
	Support for TLED100 module added
	Taiwan language updated


Messagin version 1.11RC3
        Alert mails
          Mails to multiple recipients for the same tank fixed

        Contineous mails
          Mails to multiple recipents with the same or different time schedule fixed.
	  Its own mail subject line with tank number

	Reminder
	  Controlled by the reminder setting of the tank contact so the Reminder parameter
	  in the Messgin.ini file is obsolete fro 1.11RC1 and onwards and left there for backward
	  compability.

          0 = No reminder to this contact
          1 = Send reminder to this contact          
     
	Improved logging.
	  Flag h added for message history messages

	Messaging history
	  Now also adds multiple sent messages to the history.
	  
	  FIFO size control of the number of stored message results. Handle by parameter
	  [System] FIFO in the Messagin.ini file.


KP10011RC1.bin, KP100.ocx version 1.11RC1
	Support Enable/Disable reader inputs for prompts not set in properties sections 1 - 4
	

PLC10011RC1.bin and TCM10011RC1.bin
	Trigger added for port output change to get better
	real-time reaction in graphics.


TLED100.ocx version 1.11RC8
	Support for TLED100 module (Tank LED)
	OBSERVE!
		Must be manually registered by the regsvr32.exe.

	Improved functionality
	LED properties PPU disabled
	Manual scroll timout properly stored


Reg_x32_TLED100.bat (For x32 systems)
Reg_x64_TLED100.bat (For x64 systems)
	A batch file for registrating the TLED100.ocx.
	  Put it in the Lubemast folder.
	  Right-click it and select "Run as Administrator".
          A window saying "Success" should pop-up.
	

TLED10011RC6.bin
	Support
	  65 tanks numbered 1-65.
	    The list of tanks are automatically populated by setting the LED address of
	    tank module ports to the address of the Tank LED.

	    If a Tank module port is set to stop sending data to the TLED or if it is renumbered
	    the old tank will remian in the list unless the tank module is rebooted after the change.

	    If a new tank are added the tank list will be updated with that tank automatically.

	    OBSERVE!
		The tank list uses the in tankmodule port set tank numberas identifier so NEVER
		set 2 or more tank module ports to the same tank number. If you do that the result
		on the TLED is unpredictable.

	  Interval circular mode
	    This mode is set by giving the "Tank interval time" (TiTime:) a
	    positive value other than 0. The value is in seconds so setting
	    it to for example to 5 will will make the TLED swich tank every 5 seconds.

	  Scroll mode
	    This mode is set by giving the "Tank interval time" (TiTime:)
	    the value 0. By pressing the <SELECT> button the first tank in the list
	    of collected tanks is shown. Then the list is scrolled by the
	    <"Arrow Up"> and <"Arrow Down"> buttons. To leave the tank list press the <RESET> button.

	Set Interval circular time or scroll mode from LED buttons as well as from keypad and PC layout

	Updates tankvolume also when contineously showing the volume for the same tank.


LED10111RC3.bin
	Cloning gives random FR/TO fixed


WinDBManager.exe version 1.11RC2
	View->Message History sorted by message number instead of message date
	Disconnects from database also on closing forms by "X" in titlebar.


Autores.exe version 1.11RC1
	Support for selection of Float or Integer PPU removed
	only support Float PPU.

	All module settings are aligned with <Factory default>
	button in module graphics.

	Meter range changed from 0.500 to 0.400

!Base.csl version 1.10RC3
	Change to function Exit() to support Try and Catch better.




How to use
-----------------------------------------------------------------------------------------------
        Shut down Engine

	Make a backup copy of the C:\LubeMast folder so you can go back and get settings you
	should transfer to the new ini files.

	Either run "Update_R10.bat" if LUBE-Master is installed in default location

	or maually

	Copy
	 DbTank.ocx
	 Engine.exe
	 Lang.lan
	 WinDb.dll
	 WinDb.ini
	 Script.dll
	 Script.ini
	 TLED100.ocx
	 WinDb.dll
	 WinDb.ini
	to the \LubeMast folder replacing the existing ones.

        Copy
	 WinDBManager.exe
	to the \LubeMast\WinDb Manager folder replacing the existing one.

	Copy
	 all .bin files
	to the \LubeMast\Chip folder replacing the existing one.
	Start Engine and then use HwFlash to flash the modules.
